Manifold Absolute Pressure Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the manifold absolute pressure (MAP) connector (2).
2. Disconnect the vacuum hose from the MAP sensor (1).
3. Remove the MAP sensor bolts (2).
4. Remove the MAP sensor with the bracket (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the MAP sensor and bracket (1) with bolts and nuts (2).

Tighten
Tighten the MAP sensor bracket bolts and nuts to 8-12 N·m (71-106 lb in).

Important: Inspect the MAP sensor vacuum hose for the tear and damages.

2. Connect the vacuum hose to the MAP sensor (1).
3. Connect the MAP connector (2).