Driver or Passenger Seat Cushion Frame Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front seat cushion. Refer to Front Seat Cushion Replacement .
3. Remove the guide rail bolts (1) and guide rail (2).
4. Remove the seat cushion cover.
5. Remove the hog rings.
6. Remove the seat cushion frame.

### Installation Procedure

1. Install the seat cushion cover with the hog rings.
2. Install the guide rail with the bolts.
3. Install the front seat cushion. Refer to Front Seat Cushion Replacement .
4. Connect the negative battery cable.