Shift Cable Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner. Refer to Air Cleaner Assembly Replacement for the 0.8L engine.
2. Remove the battery and battery tray. Refer to Battery Replacement .
3. Remove the shift cable bracket bolts (1) and bracket.
4. Remove the E-ring (2) and nut (3).
5. Separate the shift cable.
6. Remove the floor console. Refer to Front Floor Console Replacement .

Put aside the floor carpet in order to get the gear shift cable shown.

7. Remove the shift control clip (3).
8. Remove the shift control cable E-ring (1).
9. Disconnect the shift control cable (2).
10. Remove the shift cable nut.
11. Pull the cables out of the passenger compartment.
12. Remove the shift cable.

### Installation Procedure

1. Push the shift cable into the passenger compartment.
2. Install the shift cable.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nut.

Tighten
Tighten the shift cable nut to 10 N·m (89 lb in).

4. Connect the shift control cable (2).
5. Install the shift cable E-ring (1).
6. Install the shift control cable clip (3).
7. Install the floor console. Refer to Front Floor Console Replacement .
8. Install the shift cable.
9. Install the E-ring (2) and nut (3).
10. Install the shift cable bracket bolts (1) and bracket.

Tighten
Tighten the bracket bolts to 20 N·m (15 lb ft).

11. Install battery and battery tray. Refer to Battery Replacement .
12. Install the air cleaner assembly. refer to Air Cleaner Assembly Replacement for the 0.8L engine.