Lifting and Jacking the Vehicle. Chevrolet Joy 2008

For 1990-2009 cars

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

To raise the vehicle, place the lifting equipment only at the points indicated. Failure to use these precise positions may resulti in permanent vehicle body deformation. Many dealer service facilities and service stations are equipped with automotive hoists that bear upon some parts of the frame in order to lift the vheicle. If any other hoist method is used, use special care to avoid damaging the fuel tank, the fitler neck, the exhaust system, or the underbody.

### Vehicle Lifting Points

#### Front Lift

Rearward of the front tire.

#### Rear Lift

Foreward of the rear tire.

### Jacking

#### Rear Suspension Axle Lift Point

Under center of rear suspension axle lift point.

#### Center Rocker Lift Point (LH/RH)

Under center of the rocker lift point on both right and left hand sides.