Rear Brake Hose Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the wheels. Refer to Tire and Wheel Removal and Installation .

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

2. Remove the fittings (1) from the brake hose.
3. Remove the E-rings (2).
4. Plug the opening in the brake pipe to prevent fluid loss or contamination.
5. Remove the brake hose.

### Installation Procedure

1. Connect the brake lines to the brake hose.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fittings (1) and E-rings.

Tighten
Tighten the fitting to 16 N·m (12 lb ft).

Important: Use only General Motors recommended brake fluid.

3. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
4. Inspect the brake system for leaks.
5. Install the wheels. Refer to Tire and Wheel Removal and Installation .