Maintenance Schedule. Chevrolet Joy 2008

For 1990-2009 cars

## Maintenance Schedule Europe

### Normal Vehicle Use

These schedules are for vehicles that:

• | Carry passengers and cargo within recommended limits.

• | Are driven on reasonable road surfaces within legal driving limits.

• | Use the recommended fuel.

Important: Additional maintenance recommendations are in this subsection. Also refer to .

The services shown in this schedule up to 120 000 km (72,000 mi) should be performed after 120 000 km (72,000 mi) at the same intervals.

### Footnotes

The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance will not nullify the emission warranty or limit recall liability prior to the completion of the vehicles useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

I- Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R- Replace or change.

(1)- Inspect every 5 000 km (3,000 mi) and replenish engine oil, if necessary. If the vehicle is operated under severe conditions: short distance driving, extensive idling or driving in dusty conditions, change engine oil every 7 500 km (4,500 mi) or 6 months, whichever comes first.

(2)- More frequent maintenance is required if driving in dusty conditions.

(3)- Refer to Fluid and Lubricant Recommendations .

(4)- Change the brake fluid every 15 000 km (9,000 mi) if the vehicle is mainly driven under severe conditions: driving in hilly or mountainous terrain.

(5)- More frequent maintenance is required if used under severe conditions: short distance driving, extended idling, frequent low speed operation in stop-start traffic or driving in dusty conditions.

(6)- If necessary, rotate and balance wheels.

(7)- A good time to check the brakes is during tire rotation.

(8)- Inspect every 5 000 km (3,000 mi).

(9)- Rotate every 5 000 km (3,000 mi).

(10)- Inspect when abnormal condition is noted.

(11)- If a vehicle is operated under severe conditions: driving in heavy rainfall, high humidity, or dusty conditions, inspect drive belt every 5 000 km (3,000 mi) or 3 months, and change every 20 000 km (12,000 mi) or 1 year, whichever comes first.

### 1 000 km (600 mi)

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Inspect the engine oil and oil filter. Refer to footnote. (1),(3),(I)

• | Inspect the engine coolant. Refer to footnote. (3),(I).

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the handbrake. Refer to footnote. (4),(I)

• | Inspect the manual transaxle oil. Refer to footnote. (3),(I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the wheel alignment. Refer to footnote. (I)

### 15 000 km (9,000 mi) or Every 12 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs. Refer to footnote. (I)

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and the brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 30 000 km (18,000 mi) or every 24 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Replace the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and the vapor lines. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drums and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and the connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and the clearance. Refer to footnote. (I)

• | Inspect manual transaxle oil. Refer to footnote. (3)

• | Inspect clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Inspect seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 45 000 km (27,000 mi) or every 36 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Change the engine coolant. Refer to footnote. (3)

• | Replace the fuel filter.

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Replace air cleaner element. Refer to footnote. (2)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs. Refer to footnote. (I)

• | Inspect the distributor cap and rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate locks, hinges and hood latch. Refer to footnote. (I)

### 60 000 km (36,000 mi) or every 48 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Replace the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and the connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and the brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and the underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and the inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 75 000 km (45,000 mi) or Every 60 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Change the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect ignition timing. Refer to footnote. (I)

• | Replace the spark plugs.

• | Inspect the distributor cap and rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and the underbody bolts and nuts are tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 90 000 km (54,000 mi) or Every 72 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Replace the fuel filter.

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Replace air cleaner element. Refer to footnote. (2)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs. Refer to footnote. (I)

• | Inspect the distributor cap and rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and the connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and the brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and the underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and the inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 105 000 km (63,000 mi) or Every 84 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Replace the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate locks, hinges and hood latch. Refer to footnote. (I)

### 120 000 km (72,000 mi) or Every 96 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Replace the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and underbody bolts and nuts are tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

## Maintenance Schedule Except Europe

### Normal Vehicle Use

These schedules are for vehicles that:

• | Carry passengers and cargo within recommended limits.

• | Are driven on reasonable road surfaces within legal driving limits.

• | Use the recommended fuel.

Important: Additional maintenance recommendations are in this subsection. Also refer to .

The services shown in this schedule up to 100 000 km (60,000 mi) should be performed after 100 000 km (60,000 mi) at the same intervals.

### Footnotes

The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance will not nullify the emission warranty or limit recall liability prior to the completion of the vehicles useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

I- Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R- Replace or change.

(1)- Inspect every 5 000 km (3,000 mi) and replenish engine oil, if necessary. If the vehicle is operated under severe conditions: short distance driving, extensive idling or driving in dusty conditions, change engine oil every 5 000 km (3,000 mi) or 3 months, whichever comes first.

(2)- More frequent maintenance is required if driving in dusty conditions.

(3)- Refer to Fluid and Lubricant Recommendations .

(4)- Change the brake fluid every 15 000 km (9,000 mi) if the vehicle is mainly driven under severe conditions: driving in hilly or mountainous terrain.

(5)- More frequent maintenance is required if used under severe conditions: short distance driving, extended idling, frequent low speed operation in stop-start traffic or driving in dusty conditions.

(6)- If necessary, rotate and balance wheels.

(7)- A good time to check the brakes is during tire rotation.

(8)- Inspect every 5 000 km (3,000 mi).

(9)- Rotate every 5 000 km (3,000 mi).

(10)- Inspect when abnormal condition is noted.

(11)- If a vehicle is operated under severe conditions: driving in heavy rainfall, high humidity, or dusty conditions, inspect drive belt every 5 000 km (3,000 mi) or 3 months, and change every 20 000 km (12,000 mi) or 1 year, whichever comes first.

### 1 000 km (600 mi)

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Inspect the engine oil and oil filter. Refer to footnote. (1),(3),(I)

• | Inspect the engine coolant. Refer to footnote. (3),(I).

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the handbrake. Refer to footnote. (4),(I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the wheel alignment. Refer to footnote. (I)

### 10 000 km (6,000 mi) or Every 6 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the spark plugs. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and the brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 20 000 km (12,000 mi) or every 12 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs. Refer to footnote. (I)

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and the vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drums and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and the connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and the clearance. Refer to footnote. (I)

• | Inspect manual transaxle oil. Refer to footnote. (3)

• | Inspect clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Inspect seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 30 000 km (18,000 mi) or every 18 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3)

• | Inspect air cleaner element. Refer to footnote. (2)

• | Replace the spark plugs. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Replace the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including booster. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate locks, hinges and hood latch. Refer to footnote. (I)

### 40 000 km (24,000 mi) or every 24 months, whichever comes first

• | Replace the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Change the engine coolant. Refer to footnote. (3),(I)

• | Replace the fuel filter.

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Replace the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and the connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and the brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and the underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and the inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 50 000 km (30,000 mi) or Every 30 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Change the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs.

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and the underbody bolts and nuts are tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 60 000 km (36,000 mi) or Every 36 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect air cleaner element. Refer to footnote. (2)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Replace the spark plugs. Refer to footnote. (I)

• | Inspect the distributor cap and rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and the connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and the brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and the underbody bolts and nuts tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and the inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 70 000 km (42,000 mi) or Every 42 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Replace the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the spark plugs.

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4),(I)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including booster. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Lubricate locks, hinges and hood latch. Refer to footnote. (I)

### 80 000 km (48,000 mi) or Every 48 months, whichever comes first

• | Replace the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Replace the engine coolant. Refer to footnote. (3),(I)

• | Replace the fuel filter.

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Replace the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Inspect the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and underbody bolts and nuts are tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)

### 90 000 km (54,000 mi) or Every 54 Months, Whichever Comes First

• | Inspect the alternator-belt. Refer to footnote. (I),(11)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I),(11)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Replace the spark plugs.

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the PCV system. Refer to footnote. (I)

• | Inspect the timing belt. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including booster. Refer to footnote. (I)

• | Change the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect the chassis and underbody and nuts tight/secure. Refer to footnote. (I)

• | Inspect tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate tires. Refer to footnote. (7),(9)

• | Inspect wheel alignment. Refer to footnote. (10)

• | Inspect steering wheel and linkage. Refer to footnote. (I)

• | Inspect power steering fluid and lines. Refer to footnote. (I)

• | Inspect drive shaft boots. Refer to footnote. (I)

• | Lubricate locks, hinges and hood latch. Refer to footnote. (I)

### 100 000 km (60,000 mi) or Every 60 months, whichever comes first

• | Inspect the alternator-belt. Refer to footnote. (I)

• | Inspect the power steering, and A/C compressor belt. Refer to footnote. (I)

• | Change engine oil and filter, or every 3 months, whichever occurs first.

| An Emission Control Service.

• | Inspect the cooling system hoses and connections. Refer to footnote. (I)

• | Inspect the engine coolant. Refer to footnote. (3),(I)

• | Inspect the fuel lines and connections. Refer to footnote. (I)

• | Inspect the air cleaner element. Refer to footnote. (2),(I)

• | Inspect the ignition timing. Refer to footnote. (I)

• | Inspect the spark plugs.

• | Inspect the distributor cap and the rotor. Refer to footnote. (I)

• | Inspect the high-tension cable. Refer to footnote. (I)

• | Inspect the valve clearance. Refer to footnote. (I)

• | Inspect the charcoal canister and vapor lines. Refer to footnote. (I)

• | Inspect the exhaust pipes and mountings. Refer to footnote. (I)

• | Change the brake fluid. Refer to footnote. (3),(4)

• | Inspect the front brake pads and disc. Refer to footnote. (I)

• | Inspect the brake drum and linings. Refer to footnote. (I)

• | Inspect the handbrake. Refer to footnote. (I)

• | Inspect the brake line and connections, including the booster. Refer to footnote. (I)

• | Inspect the rear hub bearing and clearance. Refer to footnote. (I)

• | Inspect the manual transaxle oil. Refer to footnote. (3)

• | Inspect the clutch and brake pedal free play. Refer to footnote. (I)

• | Inspect that the chassis and underbody bolts and nuts are tight/secure. Refer to footnote. (I)

• | Inspect the tire condition and inflation pressure. Refer to footnote. (6),(8)

• | Rotate the tires. Refer to footnote. (7),(9)

• | Inspect the wheel alignment. Refer to footnote. (10)

• | Inspect the steering wheel and linkage. Refer to footnote. (I)

• | Inspect the power steering fluid and lines. Refer to footnote. (I)

• | Inspect the drive shaft boots. Refer to footnote. (I)

• | Inspect the seat belts, buckles and anchors. Refer to footnote. (I)

• | Lubricate the locks, hinges and hood latch. Refer to footnote. (I)