Scan Tool Output Controls. Chevrolet Joy 2008

For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selections | Description
--- | --- | ---
ABS Lamp Test | Lamp Tests | Commands the ABS Indicator ON and OFF
Automated Bleed | -- | Used in order to bleed the ABS hydraulics. Refer to Antilock Brake System Automated Bleed Procedure.
Brake Warning Lamp | Lamp Tests | Used in order to bleed the ABS hydraulics
Left Front Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Left Rear Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Pump Motor Test | -- | Commands the pump motor ON and OFF
Right Front Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Right Rear Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF