Fuel Filter Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Notice: Refer to Fuel Pressure Notice in the Preface section.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Disconnect the inlet/outlet fuel lines by pushing the line connector lock and pulling off the hose of the fuel filter tube.
3. Remove the fuel filter from the fuel tank.

### Installation Procedure

1. Install the new fuel filter into the retaining clamp. Note the flow direction.
2. Connect the inlet/outlet lines. Secure the lines with the connector lock.
3. Perform a leak test of the fuel filter.