Temperature Control Cable Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Slide the cable eyelet off the post on the temperature door lever.
3. Disconnect the cable retainer from the heater/air distributor case assembly.
4. Remove the control assembly. Refer to Heater and Air Conditioning Control Replacement .
5. Remove the temperature control cable.

### Installation Procedure

1. Install the temperature control cable.
2. Install the control assembly. Refer to Heater and Air Conditioning Control Replacement .
3. Install the temperature control cable eyelet to the post on the temperature door lever.
4. Snap the cable retainer to the A/C module.

Caution: Refer to Battery Disconnect Caution in the Preface section.

5. Connect the negative battery cable.