Unable to Run in All Ranges. Chevrolet Joy 2008

For 1990-2009 cars

#### Unable to Run in All Range

Checks | Causes
--- | ---
Incorrect ATF level adjustment | Refer to Transmission Fluid Check .
Incorrect select linkage adjustment | Refer to Park/Neutral Position Switch Replacement .

Low line pressure

Disassemble transmission and inspect:

• | Damage to each of the gears

- | Output gear

- | Idle gear

- | Differential gear

• | Torque converter

• | Operation of the parking mechanism

Broken or damage oil pump | Seized or broken pump gears
Error in control valve spool sliding | Damaged, leaking or misaligned