Front Side Door Window Channel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front door seal trim from the front door. Refer to Door Water Deflector Replacement .
2. Remove the outside rearview mirror from the front door. Refer to Outside Rearview Mirror Replacement .
3. Remove the screws (1) on the guide rail.
4. Remove the inside bolts (4).
5. Remove the outside bolts (3).
6. Remove the division bar (2).
7. Remove the guide rail from the door.
8. Remove the glass run (1).

### Installation Procedure

1. Install the glass run.
2. Install the division bar with the bolts and the screws.
3. Install the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Install the front door seal trim. Refer to Door Water Deflector Replacement .