Rear Side Door Outside Handle Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear door lock. Refer to Rear Door Lock Replacement .
3. Remove the outside rear door handle bolts (2).
4. Remove the outside rear door handle (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outside rear door handle (1) with the bolts (2).

Tighten
Tighten the bolts to 4.5 N·m (40 in lb).

2. Install the rear door lock. Refer to Rear Door Lock Replacement .
3. Connect the negative battery cable.