Headlining Trim Panel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the sun visors. Refer to Sunshade Replacement .
3. Remove the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement .
4. Pry off the windshield pillar garnish molding trim panel. Refer to Windshield Pillar Garnish Molding Replacement .
5. Pry off the upper center pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
6. Pry off the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
7. Remove the passenger assist handle and the coat hook. Refer to Assist Handle and Rear Coat Hook Replacement .
8. Remove the sunroof molding, if equipped. Refer to Sunroof Replacement .
9. Take off the tailgate opening weatherstrip. Refer to Cargo Area Rear Trim Panel Replacement .
10. Remove the headliner clips (1) and the headliner (2).

### Installation Procedure

1. Install the headliner and clips.
2. Install the tailgate opening weatherstrip. Refer to Cargo Area Rear Trim Panel Replacement .
3. Install the sunroof molding, if equipped. Refer to Sunroof Replacement .
4. Install the passenger assist handle and the coat hook. Refer to Assist Handle and Rear Coat Hook Replacement .
5. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
6. Install the upper center pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
7. Install the windshield pillar garnish molding trim panel. Refer to Windshield Pillar Garnish Molding Replacement .
8. Install the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement .
9. Install the sun visors. Refer to Sunshade Replacement .
10. Connect the negative battery cable.