Instrument Cluster System Check. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Normal Result | Abnormal Results*
--- | --- | --- | ---

1

Turn the ignition switch to the ON position.

• | The engine coolant temperature (ECT) gauge indicates the current engine coolant temperature.

• | The fuel gauge indicates the approximate fuel level.

• | The oil pressure indicator illuminates.

• | Engine Coolant Temperature Gauge Always Cold

• | Engine Coolant Temperature Gauge Always Hot

• | Engine Oil Pressure Indicator Inoperative

• | Engine Oil Pressure Indicator Always On

• | Fuel Gauge Always Indicates Empty

• | Fuel Gauge Always Indicates Full

• | Fuel Gage Inaccurate or Inoperative

2

Start the engine.

• | The oil pressure indicator turns off

• | The tachometer indicate the engine speed.

• | Engine Oil Pressure Indicator Always On

• | Engine Oil Pressure Indicator Inoperative

3

Run the engine until the normal operating temperature is reached.

The ECT gauge indicates current ECT.

• | Engine Coolant Temperature Gauge Always Cold

• | Engine Coolant Temperature Gauge Always Hot

• | Engine Coolant Temperature Gage Inaccurate or Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.