Oil Level Indicator and Tube Installation. Chevrolet Metro 2000

For 1990-2009 cars

1. Install a new guide tube oil seal to the guide tube (1).
2. Install the guide tube to the oil pump.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Secure the guide tube with one bolt.

Tighten
Tighten the guide tube bolt to 11 N·m (97 lb in).