Instrument Cluster System Check. Chevrolet Metro 1998

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

Turn the ignition switch to the ON position.

• | The engine coolant temperature (ECT) gauge indicates the current engine coolant temperature.

• | The fuel gauge indicates the approximate fuel level.

• | The oil pressure indicator lights.

• | Engine Coolant Temperature Gauge Always Cold

• | Engine Coolant Temperature Gauge Always Hot

• | ENGINE OIL PRESSURE Message Inoperative

• | ENGINE OIL PRESSURE Message Inoperative

• | Fuel Gauge Always Indicates Empty

• | Fuel Gauge Always Indicates Full

• | Fuel Gage Inaccurate or Inoperative

2

Start the engine.

• | The oil pressure indicator goes out.

• | The tachometer (if equipped) indicate the engine rpm.

• | ENGINE OIL PRESSURE Message Always On

• | ENGINE OIL PRESSURE Message Inoperative

3

Run the engine until attaining the normal operating temperature.

The ECT gauge indicates current ECT.

• | Engine Coolant Temperature Gauge Always Cold

• | Engine Coolant Temperature Gauge Always Hot

• | Engine Coolant Temperature Gage Inaccurate or Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.