Ignition Coil Module Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Disconnect the ignition control module (igniter) (1) electrical connector.
2. Remove two screws and the ignition control module (igniter) from the mounting bracket.

### Installation Procedure

1. Install the ignition control module (igniter) (1) to the mounting bracket. Secure with the 2 screws.
2. Connect the ignition control module (igniter) electrical connector.

### Noise Suppressor Filter

#### Removal Procedure

1. Remove the noise suppressor filter (2). The noise suppressor filter is taped to the harness between the ignition coil and the ignition coil module.
2. Disconnect the noise suppressor filter electrical connector.

#### Installation Procedure

1. Connect the noise suppressor filter electrical connector.
2. Install the noise suppressor filter (2) to the harness. Secure with tape.