Front Bumper Fascia Support Replacement. Chevrolet Metro 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper valance panel, if equipped. Refer to Front Bumper Valance Panel Replacement .
2. Remove the following components from the vehicle:

• | The 3 screws (2) that secure the front bumper fascia bracket

• | The front bumper fascia bracket (1)

### Installation Procedure

1. Install the front bumper fascia bracket (1) to the vehicle. Secure the bracket with 3 screws (2).
2. Install the front bumper valance panel, if removed. Refer to Front Bumper Valance Panel Replacement .