High Mount Stop Lamp Replacement. Chevrolet Metro 2000

For 1990-2009 cars

## High Mount Stop Lamp Replacement 2 Door

### Removal Procedure

1. Open the liftgate (1).
2. Remove the following components from the high mounted stoplamp housing (2):

• | The 2 screws (3)

• | The high mounted stoplamp cover (4)

3. Remove the high mounted stoplamp bulb (1) from the stoplamp cover (3), if necessary.
4. Remove the following components from the liftgate:

• | The 2 screws

• | The high mounted stoplamp housing

### Installation Procedure

1. Install the high mounted stoplamp housing to the liftgate. Secure the housing with the 2 screws.
2. Install the high mounted stoplamp bulb (1) to the stoplamp cover (3), if removed.
3. Install the high mounted stoplamp cover (4) to the stoplamp housing (2). Secure the cover with the 2 screws (3).
4. Close the liftgate

## High Mount Stop Lamp Replacement 4 Door

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the high mounted stoplamp sockets (4,7) from the underside of the rear compartment shelf (5).
3. Remove the high mounted stoplamp bulbs (1,2) from the sockets (4,7), if necessary.
4. Remove the screw that retains each side of the stoplamp (1).
5. Remove the high mounted stoplamp (1) from the vehicle.

### Installation Procedure

1. Insert the hooks into the rear window trim panel. Install the high mounted stoplamp (1) to the trim panel (2). Secure the stoplamp with the 2 screws.
2. Install the high mounted stoplamp bulbs (1,2) to the high mounted stoplamp sockets (4,7), if necessary.
3. Install the stoplamp socket (4,7) to the underside of the rear compartment shelf.
4. Close the rear compartment lid.