One-Way Clutch Overhaul. Chevrolet Metro 2000

For 1990-2009 cars

### Removal

Important: Do not disassemble the one-way clutch except for diagnostic or inspection purposes. If you find any damage or abnormal wear, replace the one-way clutch as an assembly.

1. Remove both the inner one-way clutch snap ring and the outer one-way clutch snap ring from the one-way clutch race.
2. Remove the one-way clutch from the one-way clutch race.

### Installation

1. Inspect the one-way clutch sprags and race for any abnormal wear or damage.

Install the one-way clutch into the one-way clutch race.

2. Install both the inner and the outer one-way clutch snap rings into the race.