Lighting Systems Components. Chevrolet Metro 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Backup Lamp Switch (Manual Transaxle) | Left side of the engine compartment, top of transaxle | Lighting Systems Component Views | Lighting Systems Connector End Views
Center High-Mounted Stoplamp (CHMSL) | Bottom of rear window | -- | Lighting Systems Connector End Views
Daytime Running Lamps (DRL) Control Module | Behind the left side of the IP | Lighting Systems Component Views | Lighting Systems Connector End Views
Diode Module | Behind the center IP, taped to the IP harness | Lighting Systems Component Views | Engine Controls Connector End Views
Illumination Controller | In the IP, left of the steering column | -- | Lighting Systems Connector End Views
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
LH Front Door Jamb Switch | Left front door frame, in lower rear corner | Lighting Systems Component Views | --
Luggage Compartment Lamp (4-Door) | Center of the luggage compartment, under rear window shelf | Lighting Systems Component Views | Lighting Systems Connector End Views
Luggage Compartment Lamp Switch (4-Door) | Center rear of the luggage compartment mounted to deck lid striker | -- | --
Parking Brake Switch | Passenger compartment, behind manual selector | Instrument Panel, Gages, and Console Component Views | --
Radio | Center of the IP | -- | Entertainment Connector End Views
Rear Defogger Switch | In the IP, left of steering column | -- | Stationary Windows Connector End Views
Rear Wiper/Washer Switch (2-Door LSi) | In IP, left of the steering column | -- | Wiper/Washer Connector End Views
Relay Box | Left front engine compartment, near the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
Stoplamp Switch | Top of brake pedal | Lighting Systems Component Views | Lighting Systems Connector End Views
Transaxle Range Switch (Automatic Transaxle) | Left side of the engine compartment, mounted to top of the transaxle | -- | Automatic Transmission Connector End Views
Turn Signal/Combination Switch | On steering column | -- | Lighting Systems Connector End Views
C112 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near bulkhead | Harness Routing Views | Inline Harness Connector End Views
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C201 (14 Cavities) | Main harness to the floor harness, behind the left side of the IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C203 (13 Cavities) | I/P harness to floor harness, behind left side of the IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C207 (3 Cavities) | IP harness to dome lamp harness, right side of the upper cowl | Harness Routing Views | Inline Harness Connector End Views
C400 (10 Cavities) (4-Door) | Floor harness to luggage compartment harness, left front side of luggage compartment near the left rear speaker | Harness Routing Views | --
C402 (6 Cavities) (2-Door) | Floor harness to liftgate harness, right rear corner of vehicle | Harness Routing Views | --
G102 | Left front side of the engine compartment on the left front inner fender near battery | Harness Routing Views | --
G103 | Right front side of the engine compartment on the right front side of the inner fender | Harness Routing Views | --
G201 | Behind the left side of the kick panel | Harness Routing Views | --
G202 | Right side of the center IP behind the radio | Harness Routing Views | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G400 (2-Door) | Rear center of luggage compartment | Harness Routing Views | --
(4-Door) | Rear center of luggage compartment | Harness Routing Views | --
G401 (2-Door) | Center of the liftgate, near rear wiper motor | Harness Routing Views | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
P400 | Left rear side of the luggage compartment | -- | --
P401 | Right rear of luggage compartment | -- | --
P402 | Center rear side of the luggage compartment | Harness Routing Views | --
P403 (2-Door) | Upper right side of the liftgate | Harness Routing Views | --
S100 | Main harness, approximately 10 cm (4 in) from G103 breakout | Harness Routing Views | --
S102 | Main harness, approximately 8 cm (3.1 in) from G102 breakout | Harness Routing Views | --
S104 | Main harness, approximately 13 cm (5.1 in) from brake fluid level switch breakout | Harness Routing Views | --
S105 | Main Harness, approximately 6 cm (2.4 in) from Relay Box breakout | Harness Routing Views | --
S107 | Main Harness, approximately 22 cm (8.8 in) from P200 | Harness Routing Views | --
S113 | Main harness, approximately 6 cm (2.4 in) from the G102 breakout | Harness Routing Views | --
S117 | Main harness, at the G103 breakout | Harness Routing Views | --
S154 (Automatic Transaxle) | Engine Harness, approximately 9 cm (3.6 in) from P202 | Harness Routing Views | --
S162 | Engine harness, approximately 10 cm (4 in) from P202 | Harness Routing Views | --
S202 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C6 breakout | -- | --
S204 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C5 breakout | -- | --
S205 | Main harness, approximately 1 cm (0.375 in) from P200 | -- | --
S206 (With ABS) | Main harness, approximately 22 cm (9 in) from the stoplamp switch connector breakout | -- | --
S207 | Main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S209 | Main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S210 | Main harness, approximately 15 cm (6 in) from C208 | -- | --
S217 | IP harness, at the C200 breakout | Harness Routing Views | --
S218 | IP harness, approximately 3 cm (1.19 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S219 | IP Harness, approximately 3 cm (1.19 in) from the C200 breakout | Harness Routing Views | --
S221 | IP harness, approximately 7 cm (3 in) from the IP cluster assembly connector C2 breakout | Harness Routing Views | --
S222 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2 ) breakout | Harness Routing Views | --
S223 | Main harness, approximately 10 cm (4 in) from P200 | -- | --
S228 | IP harness, at the C200 breakout | Harness Routing Views | --
S229 | IP harness, approximately 4 cm (2 in) from the IP cluster assembly connector C1 breakout | Harness Routing Views | --
S230 | IP harness, approximately 13 cm (5.125 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views | --
S236 | IP harness, approximately 8 cm (3.125 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S238 | IP harness, approximately 3 cm (1.19 in) from the blower motor connector breakout | Harness Routing Views | --
S239 | IP harness, approximately 11 cm (4.313 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S243 | IP harness, approximately 5 cm (2 in) from the cigar lighter connector breakout | Harness Routing Views | --
S244 | Main harness, approximately 23 cm (9.06 in) from P200 | -- | --
S247 | Main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S248 | Engine harness, approximately 4 cm (2 in) from the powertrain control module (PCM) connector C1 breakout | Harness Routing Views | --
S250 | IP harness, approximately 6 cm (2.375 in) from the diode module connector breakout | Harness Routing Views | --
S252 | IP harness, approximately 4 cm (2 in) from the data link connector - (DLC-OBD 2) breakout | Harness Routing Views | --
S254 | IP harness, approximately 6 cm (2.375 in) from the C215 breakout | Harness Routing Views | --
S256 | Main harness, near the junction block connector C6 breakout | -- | --
S302 | Floor harness, approximately 10 cm (4 in) from the C201 breakout | Harness Routing Views | --
S310 (4-Door) | Floor harness, approximately 6 cm (2.375 in) from the junction block connector C8 breakout. | Harness Routing Views | --
S400 (2-Door) | Floor harness, approximately 36 cm (14.17 in) from the C402 breakout | -- | --
(4-Door) | Floor harness, approximately 39 cm (14.19 in) from the left rear combination lamp connector breakout | -- | --
S401(2-Door) | Floor harness, approximately 13 cm (5.125 in) from the G400 breakout | -- | --
(4-Door) | Floor harness, approximately 27 cm (11 in) from the left rear combination lamp connector breakout | -- | --
S402 (2-Door) | Floor harness, approximately 5 cm (2 in) from the left rear combination lamp connector breakout | -- | --
S403 (2-Door) | Floor Harness, approximately 5 cm (2 in) from G400 breakout | -- | --
S404(2-Door) | Floor harness, approximately 8 cm (3.125 in) from the G400 breakout | -- | --
(4-Door) | Floor harness, approximately 10 cm (4 in) from the luggage compartment lamp switch connector breakout | -- | --
S405(2-Door) | Floor harness, approximately 13 cm (5.125 in) from left rear combination lamp connector breakout | -- | --
(4-Door) | Floor harness, approximately 34 cm (13.375 in) from the left rear combination lamp connector breakout | -- | --
S406 (4-Door) | Floor harness, approximately 10 cm (4 in) from the left rear combination lamp connector breakout | -- | --
S407 (4-Door) | Floor harness, approximately 20 cm (8 in) from the left rear combination lamp connector breakout | -- | --
S408 (4-Door) | Floor harness, approximately 5 cm (2 in) from the C400 breakout | -- | --
S410 (2-Door) | Right rear combination lamp pigtail, approximately 8 cm (3.125 in) from P401 | -- | --
S411 | Right rear combination lamp pigtail, approximately 6 cm (2.375 in) from P401 | -- | --
S412 (2-Door) | Left rear combination lamp pigtail, approximately 8 cm (3.125 in) from P400 | -- | --
S413 | Left rear combination lamp pigtail, approximately 6 cm (2.375 in) from P400 | -- | --
S419 (4-Door) | Floor harness, approximately 21 cm (8.25 in) from the left rear door jamb switch connector breakout | -- | --