Data Link Communications Components. Chevrolet Metro 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views | Data Link Communications Connector End Views
Electronic Brake Control Module (EBCM) (With ABS) | Behind the left IP, above the junction block | Antilock Brake System Component Views | Antilock Brakes System Connector End Views
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Center of the console, in front of the manual selector | SIR Component Views | SIR Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views | Powertrain Control Module Connector End Views in Engine Controls - 1.3L or Powertrain Control Module Connector End Views or Engine Controls - 1.0 L.
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C205 (12 Cavities) | IP harness to engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views | Inline Harness Connector End Views
C210 (5 Cavities) | Supplemental inflatable restraint (SIR) harness to the IP harness, behind the left side of the IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
G105 (VIN 6) | Center rear of engine, on the intake manifold | -- | --
G203 | Junction block case ground, under the left side of the IP | -- | --
S222 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views | --
S236 | IP harness, approximately 8 cm (3.125 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S237 | IP harness, approximately 10 cm (4 in) from the radio connector breakout | Harness Routing Views | --
S240 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S245 | IP harness, approximately 12 cm (5 in) from the I/P cluster assembly connector C3 breakout | Harness Routing Views | --
S249 | IP harness, approximately 1 cm (.375 in) from the IP cluster assembly connector C2 breakout | Harness Routing Views | --