Rear Side Door Trim Panel Replacement. Chevrolet Metro 2001

For 1990-2009 cars

### Removal Procedure

1. Pull the rear door molding from the rear door (2).
2. Remove the following components from the door:

• | The screw

• | The inside handle bezel (1)

3. Remove the window regulator handle (1) by using a cloth in order to pull off the snap ring.
4. Remove the following components from the rear side door trim (4):

• | The screw

• | The rear door pull handle

5. Gently pry the door trim (4) from the door (1) by disengaging the retainers.
6. Disconnect the power window switch connector, if necessary.
7. Remove the door trim (4) from the vehicle.

### Installation Procedure

1. Connect the power window switch connector, if necessary.
2. Position the rear side door trim (4) to the rear door (1).
3. Press the door trim retainers into position.
4. Install the rear door pull handle to the door trim (4). Secure the handle with the screw.
5. Install the inside handle bezel (1). Secure the bezel with the screw.
6. Install the snap ring to the window-regulator handle (3).
7. Set the regulator handle (3) at a 45-degree angle when the rear door window is completely closed.
8. Install the regulator handle (3) to the door.
9. Install the rear door molding to the door (2).