External Leakage Check. Chevrolet Metro 2000

For 1990-2009 cars

This procedure pinpoints the location of the leak. In some cases, you may easily locate the leak. However, seepage-type leaks may be more difficult to isolate. In order to locate the seepage leaks, use the following method:

1. With the engine off, wipe dry the complete power steering system.
2. Inspect the fluid level in the reservoir. Add fluid if necessary. Refer to Checking and Adding Power Steering Fluid .
3. Add 1 oz Automatic Transmission Fluorescent Tracer Dye, GM P/N 12345796, or equivalent, to the power steering fluid.
4. START the engine.

Notice: Do not hold the steering wheel in the full turn position longer than 5 seconds, as damage to the steering pump may result.

5. Turn the steering wheel from stop to stop several times.

It is easier if an assistant operates the steering wheel while you search for seepage.

6. Using a UV lamp, inspect the power steering system in order to locate the leak.
7. Loosen the steering gear boots in order to inspect for leaks from the power steering gear.
8. Repair the leak.