Fasten Safety Belt Indicator/Chime Inoperative. Chevrolet Metro 1999

For 1990-2009 cars

Step | Action | Value | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warning System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check

2

1. Unbuckle the left side seat belt.
2. Turn the ignition switch to the ON position.
3. Using a test lamp, backprobe connector C3 of the instrument cluster assembly from cavity 11 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | The left side seat belt is unfastened. The ignition switch is in the ON position. Back probe cavity 12 of the IP cluster assembly connector C3 to ground with a test lamp. Does the test lamp light? | -- | Go to Step 5 | Go to Step 7
4 | Repair the BLK/WHT wire between S242 and the instrument panel cluster assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
5 | The seat belt is unfastened. Test for an open between the seat belt switch cavity 2 and ground. Is there continuity? | -- | Go to Step 9 | Go to Step 6
6 | Replace the seat belt buckle. Refer to Seat Belt Retractor Replacement - Left Front in Seat Belts. Is the repair complete? | -- | Go to Audible Warnings System Check | --
7 | Test the seat belt indicator bulb. Is the bulb working correctly? | -- | Go to Step 8 | Go to Step 10
8 | Replace the instrument panel cluster assembly. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges and Console. Is the repair complete? | -- | Go to Audible Warnings System Check | --
9 | Repair the GRY/RED wire between cavity 2 of the seat belt switch and Connector C3 cavity 12 of the instrument panel cluster assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
10 | Replace the seat belt indicator bulb. Refer to Instrument Cluster Bulb Replacement in Instrument Panel, Gauges and Console. Is the repair complete? | -- | Go to Audible Warnings System Check | --