Key-in-Ignition Chime On with Left Front Door Open, Key Not in Ignition. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 | Disconnect the junction block connector C2. Does the alarm continue to sound? | -- | Go to Step 3 | Go to Step 4
3 | Test for a short to voltage in the BLU/BLK wire between Connector C4 cavity 14 of the junction block and the audio alarm module cavity 4. Did you find a short to voltage? | -- | Go to Step 5 | Go to Step 6
4 | Replace the ignition key warning switch. Is the repair complete? | -- | Go to Audible Warnings System Check | --
5 | Repair the short to voltage in the BLU/BLK wire between connector C4 cavity 14 of the junction block and cavity 4 of the audio alarm module. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
6 | Inspect the audio alarm module for bad connections. If you did not find a condition, replace the audio alarm module. Refer to Audio Alarm Module Replacement . Is the repair complete? | -- | Go to Audible Warnings System Check | --