Engine Electrical Components. Chevrolet Metro 2000

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | Left side of the engine compartment | Power and Grounding Component Views in Wiring Systems | --
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal | Engine Electrical Component Views | --
Fuse Box | Left side of the engine compartment, mounted on the left inner side of the fender, behind the relay box | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Generator | Right rear side of the engine compartment, mounted to the engine | Engine Electrical Component Views | --
Ignition Switch | Right side of the steering column | -- | --
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views | Powertrain Control Module Connector End Views in Engine Controls
Starter Motor | Center rear of the engine | Engine Electrical Component Views | --
Starter Solenoid | Center rear of the engine, on the top of the starter motor | Engine Electrical Component Views | --
Transaxle Range Switch (Automatic Transaxle) | Left side of the engine compartment, mounted to the top of the transaxle | -- | Automatic Transmission Connector End Views in Automatic Transmission
C112 (16 Cavities) | Main harness to the engine harness, in the right rear side of the engine compartment, near the bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C113 (16 Cavities) | Main harness to the engine harness, in the right rear side of the engine compartment, near the bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C204 (2 Cavities) (Manual Transaxle) | Main harness to the clutch pedal position switch, behind the left side of the IP | Harness Routing Views in Wiring Systems | --
C205 (12 Cavities) | IP harness to the engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G100 | Mounted on top of the left side of the transaxle | -- | --
G101 | Left front side of the engine compartment, in front of the battery | -- | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views in Wiring Systems | --
S101 | Main harness, approximately 11 cm (4.5 in) from the breakout to the brake fluid level switch | Harness Routing Views in Wiring Systems | --
S126 | Engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views in Wiring Systems | --
S152 | Main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views in Wiring Systems | --
S160 (VIN 2) | Engine Harness, approximately 20 cm (8 in) from P202 | -- | --
S162 | Engine harness, approximately 10 cm (4 in) from P202 | Harness Routing Views in Wiring Systems | --
S202 | Main harness, approximately 8 cm (3.125 in) from the breakout of connector C6 of the junction block | -- | --
S231 | Main harness, approximately 15 (6 in) cm from P200 | -- | --
S241 | IP harness, approximately 5 cm (2 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S242 | IP harness, at the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --