PSP Switch Diagnosis. Chevrolet Metro 2000

For 1990-2009 cars
Engine Controls Components
Cell 21: Idle-Up Signals
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The power steering pressure (PSP) switch is normally open to ground. Turning the steering wheel increases power steering oil pressure. Increased oil pressure in the power steering system puts an additional load on the engine that may be noticeable at idle. The PSP switch will close before the load on the engine causes an idle condition which is undesireable. The powertrain control module (PCM) increases the throttle-valve opening in order to maintain acceptable idle quality and in order to prevent an engine stall.

The voltage signal from the PSP switch to the PCM indicates less than one volt when the PSP switch is closed. The voltage signal is near battery voltage when the PSP switch is open.

### Diagnostic Aids

A PSP switch that does not close, or a loss of ground at the PSP switch, may cause the engine to stall when power steering loads are high.

A PSP switch that does not open a signal line that is shorted to ground may affect idle quality.

A fault in the electrical circuit of the power steering pressure switch may cause an intermittent malfunction. Inspect the wiring harness and the components for any of the following conditions:

• | Backed out terminals

• | Incorrect mating of terminals

• | Broken electrical connector locks

• | Incorrectly formed terminals or damaged terminals

• | Faulty terminal-to-wire connections

• | Physical damage to the wiring harness

• | A broken wire inside the insulation

• | Corrosion of electrical connections, of splices, or of terminals

### Test Description

The numbers below refer to the step numbers in the diagnostic table.

1. The Powertrain OBD System Check prompts the technician to complete some basic checks, and to store the applicable freeze frame data on the scan tool. This creates an electronic copy of the data that was taken when the fault occurred. The scan tool stores the information for later reference.

2. This step checks for voltage from the PCM, for an open, or for a short to ground in the PSP switch signal circuit.

3. This step checks for a faulty ground connection at the power steering pump or for a faulty PSP switch.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check

2

1. Install a scan tool.
2. Start the engine.
3. Run the engine until normal operating temperature is reached.
4. Turn OFF all accessories.
5. Monitor the PSP switch on the scan tool.
6. Turn the steering wheel all the way to the right and all the way to the left.

Did the scan tool indicate ON when the steering wheel was turned all the way in either direction?

--

Go to Diagnostic Aids

Go to Step 3

3

1. Turn ON the ignition, leaving the engine OFF.
2. Disconnect the PSP switch electrical connector.
3. Measure the voltage from the harness side of the PSP switch connector to ground with a DMM.

Was the voltage near the specified value?

B+

Go to Step 4

Go to Step 5

4

1. Connect a test lamp to B+.
2. Probe the switch side of the PSP switch connector with the test lamp.
3. Start the engine.
4. Observe the test lamp while turning the steering wheel all the way to the right and all the way to the left.

Was the test lamp ON when the steering wheel was turned all the way to the right or all the way to the left?

--

Go to Diagnostic Aids

Go to Step 6

5

1. Check for an open or for a short to ground in the PSP signal circuit between the PCM and the PSP switch.
2. Repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Was a repair necessary?

--

Go to Step 9

Go to Step 8

6

1. Check for a faulty ground connection at the power steering pump.
2. Repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Was a repair necessary?

--

Go to Step 9

Go to Step 7

7 | Replace the PSP switch. Refer to PSP Switch Replacement . Is the action complete? | -- | Go to Step 9 | --
8 | Replace the PCM. Is the action complete? | -- | Go to Step 9 | --
9 | Operate the vehicle within the conditions under which the original symptom was noted. Does the system now operate correctly? | -- | System OK | Go to Diagnostic Aids