ABS Components. Chevrolet Metro 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake fluid Level Switch | In Brake Fluid Reservoir | 8A-201-02 | --
Electronic Brake Control Module (EBCM) (With ABS) | Behind LH I/P above Junction Block | A-201-03 | --
Electronic Brake Control Module (EBCM) (With ABS) - C1 (24 Cavities) | Main Harness to EBCM, behind LH I/P above Junction Block | 8A-201-03 | --
Electronic Brake Control Module (EBCM) (With ABS) - C2 (8 Cavities) | Main Harness to EBCM, behind LH I/P above Junction Block | 8A-201-03 | --
Fuse Box | LH Engine Compartment mounted on LH Inner Fender behind Relay Box | 8A-201-12 | --
Fuse Box - C3 (1 Cavitiy) | Main Harness to Fuse Box, below Fuse Box | 8A-201-13 | --
Instrument Panel Cluster Assembly | LH I/P | 8A-201-04 | --
Instrument Panel Cluster Assembly - C1 (16 Terminals) | I/P Harness to I/P Cluster Assembly, behind upper RH corner of I/P Cluster Assembly | 8A-201-04 | 8A-81-02
Instrument Panel Cluster Assembly - C3 (13 Terminals) | I/P Harness to I/P Cluster Assembly, behind upper LH corner of I/P Cluster Assembly | 8A-201-04 | 8A-81-04
Junction Block | Behind LH I/P | 8A-201-03 | --
Junction Block - C4 (20 Cavities) | I/P Harness to Junction Block, behind LH I/P | 8A-201-04 | 8A-202-00
Junction Block - C5 (6 Cavities) | Main Harness to Junction Block, behind LH I/P | 8A-201-03 | 8A-202-13
Junction Block - C6 (18 Cavities) | Main Harness to Junction Block, behind LH I/P | 8A-201-03 | 8A-202-01
Lamp Driver Relay (With ABS) | Behind LH I/P, left of Steering Column near Electronic Brake Control Module (EBCM) | 8A-201-03 | 8A-202-14
Left Front Wheel Speed Sensor (With ABS) | Mounted in LH Front Steering Knuckle | 8A-201-15 | --
Left Rear Wheel Speed Sensor (With ABS) | Mounted in LH Rear Suspension Knuckle | 8A-201-15 | --
LH Front ABS Solenoid | LH Rear Engine Compartment attached to ABS Motor Pack Assembly | 8A-201-12 | --
Relay Box | LH Front Engine Compartment near Battery | 8A-201-12 | 8A-202-11
Right Front Wheel Speed Sensor (With ABS) | Mounted in RH Front Steering Knuckle | 8A-201-15 | --
Right Rear Wheel Speed Sensor (With ABS) | Mounted in RH Rear Suspension Knuckle | 8A-201-15 | --
RH Front ABS Solenoid | LH Rear Engine Compartment attached to ABS Motor Pack Assembly | 8A-201-12 | --
Stop Lamp Switch (Manual Transaxle) | Top of Brake Pedal | 8A-201-03 | --
Stop Lamp Switch (Automatic Transaxle) | Top of Brake Pedal | 8A-201-03 | 8A-202-14
C114 (2 Cavities) (With ABS) | Main Harness to LH Front Wheel Speed Sensor Jumper Harness, LH Rear Engine Compartment near Strut Tower | -- | --
C115 (2 Cavities) (With ABS) | Main Harness to RH Front Wheel Speed Sensor Jumper Harness, RH Rear Engine Compartment near Strut Tower | -- | --
C200 (12 Cavities) | Main Harness to I/P Harness, behind LH I/P near Junction Block | 8A-201-04 | 8A-202-06
C201 (14 Cavities) | Main Harness to Floor Harness, behind LH I/P near Junction Block | 8A-201-03 | 8A-202-07
C304 (2 Cavities) (With ABS) | Floor Harness to RH Rear Wheel Speed Sensor Jumper Harness, under RH side of Rear Passenger Seat | 8A-201-06 | --
C305 (2 Cavities) (With ABS) | Floor Harness to LH Rear Wheel Speed Sensor Jumper Harness, under LH side of Rear Passenger Seat | 8A-201-06 | --
G102 | LH Front Engine Compartment on LH Front Inner Fender near Battery | -- | --
G201 | Behind LH Kick Panel | 8A-201-03 | --
P100 (With ABS) | LH Rear Engine Compartment on Strut Tower | -- | --
P101 (With ABS) | RH Rear Engine Compartment on Strut Tower | -- | --
P200 | LH Rear Engine Compartment on Bulkhead near Brake Master Cylinder | -- | --
P301 | Under RH side of Rear Passenger Seat | -- | --
P302 | Under LH side of Rear Passenger Seat | -- | --
S124 (With ABS) | Main Harness, approximately 5 cm from Front ABS Solenoids breakout | -- | --
S206 (With ABS) | Main Harness, approximately 22 cm from Stoplamp Switch Connector breakout | -- | --
S207 | Main Harness, approximately 12 cm from G201 breakout | -- | --
S208 (With ABS) | Main Harness, approximately 12 cm from G201 breakout | -- | --
S209 | Main Harness, approximately 2 cm from G201 breakout | -- | --
S213 | Main Harness, approximately 8 cm from P200 | -- | --
S215 (With ABS) | Main Harness, approximately 4 cm from Junction Block Connector C6 breakout | -- | --
S223 | Main Harness, approximately 10 cm from P200 | -- | --
S241 | I/P Harness, approximately 5 cm from I/P Cluster Assembly connector C3 breakout | 8A-201-04 | --
S242 | I/P Harness, at I/P Cluster Assembly connector C3 breakout | 8A-201-04 | --
S247 | Main Harness, approximately 18 cm from P200 | -- | --
S249 | I/P Harness, approximately 1 cm from I/P Cluster Assembly connector C2 breakout | 8A-201-04 | --