Wipers Delay Mode Inoperative. Chevrolet Metro 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 | Backprobe the junction block connector C3 with a test lamp from cavity 9 to B+. Does the test lamp light? | -- | Go to Step 3 | Go to Step 4
3 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
4 | Test for an open in the BLK wire between the combination switch and the junction block. Was an open found? | -- | Go to Step 6 | Go to Step 5
5 | Replace the junction block. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --