Wipers On Mode Inoperative - Rear. Chevrolet Metro 2001

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check

2

1. Turn the ignition switch to the ON position.
2. Backprobe the rear wiper/washer switch connector with a test lamp from cavity 4 to ground.

Does the test lamp light?

--

Go to Step 4

Go to Step 3

3 | Test for an open in the YEL/BLU wire between the junction block and the rear wiper/washer switch. Was an open found? | -- | Go to Step 5 | Go to Step 6
4 | Replace the rear wiper/washer switch. Refer to Rear Window Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
5 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
6 | Replace the junction block. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --