License and Tail Lamps Inoperative. Chevrolet Metro 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check .

2

1. Turn the light switch to the PARK position.
2. Backprobe the junction block connector C8 using J 35616-200 from cavity 2 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Repair the open in the RED/YEL wire between S405 and the junction block. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check . | --
4 | Test for an open in the RED/YEL wire between the junction block and S204. Was an open found? | -- | Go to Step 6 | Go to Step 5
5 | Replace the junction block. Is the repair complete? | -- | Go to Exterior Lights System Check . | --
6 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check . | --