Rear Window Wiper Arm Replacement. Chevrolet Metro 2001

For 1990-2009 cars

### Removal Procedure

Important: Observe the location of the wiper arm. This will ensure correct installation.

1. Lift the plastic nut cover (2) in order to gain access to the rear wiper arm retaining nut.
2. Remove the wiper arm retaining nut.
3. Remove the wiper arm (5) from the wiper linkage (7).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the wiper arm (5) to the wiper linkage (7). Secure the wiper arm with the retaining nut.

Tighten
Tighten the wiper arm retaining nut to 20 N·m (15 lb ft).

2. Place the plastic nut cover (2) over the wiper arm retaining nut.