Blower Motor Resistor Replacement. Chevrolet Metro 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the powertrain control module. Refer to Powertrain Control Module Replacement in Engine Controls-1.0L or Powertrain Control Module Replacement in Engine Controls-1.3L.
2. Disconnect the blower motor resistor electrical connector.
3. Remove the following components from the blower case:

• | The 1 screw (3)

• | The blower motor resistor (2)

### Installation Procedure

1. Install the resistor (2) to the blower case.

Secure the resistor with 1 screw (3).

2. Connect the blower motor resistor electrical connector.
3. Install the PCM. Refer to Powertrain Control Module Replacement in Engine Controls-1.0L or Powertrain Control Module Replacement in Engine Controls-1.3L.

### Removal Procedure

1. Remove the powertrain control module (PCM). Refer to Powertrain Control Module Replacement -1.0L, or Powertrain Control Module Replacement -1.3L in Engine Controls.
2. Disconnect the electrical connector of the blower-motor resistor.
3. Remove 1 screw (3) and the blower-motor resistor (2) from the blower case (1).

### Installation Procedure

1. Install the resistor (2) to the blower case (1). Secure the resistor with the 1 screw (3).
2. Connect the electrical connector of the blower-motor resistor electrical connector.
3. Install the PCM. Refer to Powertrain Control Module Replacement 1.0L or Powertrain Control Module Replacement 1.3L in Engine Controls.