Rear Seat Back Cushion Latch Striker Replacement. Chevrolet Metro 1999

For 1990-2009 cars

## Rear Seat Back Cushion Latch Striker Replacement 2 Door

### Removal Procedure

1. Position the rear seat back cushion forward.
2. Remove the rear strut tower trim from the rear compartment trim panel.
3. Remove the following components from the vehicle:

• | The bolt (1)

• | The nut (3)

• | The seat back lock striker (2)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear seat back striker (2) to the vehicle. Secure the striker with the nut (3) and with the bolt (1).

Tighten
Tighten the nut and the bolt that retain the rear seat back striker to 25 N·m (18 lb ft).

2. Install the rear strut tower trim to the rear compartment trim panel.
3. Return the rear seat back to the up position.