Timing Belt Removal. Chevrolet Metro 1998

For 1990-2009 cars

1. Remove the eight bolts and one nut that secure the timing belt cover.
2. Remove the timing belt cover (12).

Important: Before removing the timing belt, align the upper and the lower timing marks by turning the crankshaft.

3. Ensure that the upper timing marks (1 and 2) are aligned.
4. Ensure that the lower timing marks (1 and 2) are aligned.
5. Loosen the timing belt tensioner bolt (2) and the stud (1).
6. Remove the belt from the crankshaft timing belt pulley and the camshaft timing belt pulley after pushing up the tensioner plate fully with your finger.