Front Side Door Window Belt Inner Sealing Strip Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Release the 5 tabs that retain the inner sealing strip (1) to the door trim (2).

### Installation Procedure

1. Insert the tabs of the inner sealing strip (1) into the door trim (2). Fold the tabs over.
2. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .