Instrument Panel Center Air Outlet Deflector Replacement. Chevrolet Metro 2000

For 1990-2009 cars

### Removal Procedure

1. Gently pry-out the center vent garnish (4) with a small flat screwdriver.
2. Remove the IP center outlet duct. Refer to IP Air Outlet Ducts Replacement in Heating, Ventilation and Air Conditioning or HVAC Systems - Manual.
3. Remove the 3 screws and the center vent louver (1) from the IP.

### Installation Procedure

1. Install the center vent louver (1) to the IP. Secure the louver with the 3 screws.
2. Install the center vent garnish panel (4) to the IP. Push the panel in until the panel fully engages.
3. Install the IP center outlet duct. Refer to IP Air Outlet Ducts Replacement in Heating, Ventilation and Air Conditioning or HVAC Systems - Manual.