Turn Signal and Hazard Lamps Inoperative. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Was the Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check

2

1. Press the hazard switch to the ON position.
2. Backprobe the junction-block connector C 3 with a test lamp from cavity 4 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Exterior Lights System Check | --
4 | Connect a fused jumper from the C 3 cavity 3 of the junction-block connector to cavity 1. Do the right side turn signals flash? | -- | Go to Step 5 | Go to Step 6
5 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Exterior Lights System Check | --
6 | Replace the turn relay. Is the repair complete? | -- | Go to Exterior Lights System Check | --