Key-in-Ignition Chime On with Left Front Door Closed. Chevrolet Metro 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 | Disconnect the LH door jamb switch connector. Does the warning alarm continue to sound? | -- | Go to Step 4 | Go to Step 3
3 | Replace the LH door jamb switch. Is the repair complete? | -- | Go to Audible Warnings System Check | --
4 | Test for a short to ground using a J 39200 in the BLK/BLU wire between cavity 6 and the LF door jamb switch connector. Was a short to ground condition found? | -- | Go to Step 5 | Go to Step 6
5 | Repair the short to ground in the BLK/BLU wire between cavity 6 and the LF door jamb switch connector. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
6 | Replace the audio alarm module. Refer to Audio Alarm Module Replacement . Is the repair complete? | -- | Go to Audible Warnings System Check | --