CAMPAIGN: LEFT REAR STRUT TO AXLE CARRIER BOLTS. Chevrolet Nova 1988

For 1990-2009 cars

# CAMPAIGN: LEFT REAR STRUT TO AXLE CARRIER BOLTS

#### Model and Year: 1988 CHEVROLET NOVA

General Motors has determined that certain 1988 Chevrolet Nova model vehicles may exhibit low torque on the left rear strut to carrier bolts.

To correct this condition, the left rear strut to carrier bolts must be checked for proper torque.

#### VEHICLES INVOLVED

Involved are certain 1988 Chevrolet Nova model vehicles produced within the following VIN breakpoints:

PLANT FROM THROUGH ----- ---- -------

Fremont JZO82185 JZO92941

#### DEALER CAMPAIGN RESPONSIBILITY

Dealers are to service all vehicles subject to this campaign at no charge to owners, regardless of mileage, age of vehicle, or ownership, from this time forward.

Owners of any of these vehicles that may possibly have been sold from your new vehicle inventory are to be contacted by the dealer, and arrangements made to make the required correction according to instructions contained in this bulletin.

#### PARTS INFORMATION

No parts are required to complete this campaign.

#### SERVICE PROCEDURE

1. Raise rear of vehicle and support body with stands or raise vehicle on hoist.

2. Remove left rear wheel/tire assembly.

3. Torque two left rear strut to axle carrier nuts (rear) while holding bolts (front) with a wrench (see Illustration)(Figure 1). Torque to 105 lbs. ft. (142 Nm).

4. Reinstall left rear wheel/tire assembly. Torque wheel nuts to 76 lbs. ft. (105 Nm).

5. Install Campaign Identification Label.

#### CAMPAIGN IDENTIFICATION LABEL (Figure 2)

Each vehicle corrected in accordance with the instructions outlined in this Product Campaign Bulletin will require a "Campaign Identification Label." Each label provides a space to include the five (5) digit dealer code of the dealer performing the campaign service. This information may be inserted with a typewriter or a ball point pen.

Each "Campaign Identification Label" is to be located on the radiator core support in an area which will be visible when the vehicle is brought in for periodic servicing by the owner. Apply "Campaign Identification Label" only on a clean dry surface.

#### CLAIM INFORMATION

Submit a Product Campaign Claim with the information indicated below:

* FAILED PARTS LABOR LAB OTH REPAIR PERFORMED PC PART NO. ALLOW FC OP HRS HRS ---------------- -- -------- ----- -- ----- --- ---

Torque Left Rear 00 V4880 0.3 0.1 Strut to Carrier Bolts

* Campaign Administrative Allowance

Dealers will automatically receive the correct labor and material allowance based on the labor operation performed.

Refer to the Chevrolet Claims Processing Manual for details on Product Campaign Claim Submission.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.