HIGH ALTITUDE CO EXHAUST EMISSIONS FED EMISSIONS UNITS. Chevrolet Nova 1988

For 1990-2009 cars

# HIGH ALTITUDE CO EXHAUST EMISSIONS FED EMISSIONS UNITS

DCS MESSAGE

PRODUCT EMISSION CAMPAIGN 88C30 HIGH ALTITUDE CO EXHAUST EMISSIONS FEDERAL EMISSIONS UNITS ONLY 1.6L ENGINE (LC9)

EFFECTIVE IMMEDIATELY PLEASE STOP PERFORMING AND/OR SCHEDULING OWNERS TO PERFORM PRODUCT CAMPAIGN 88C30. REPORTS OF IDLE DEGRADATION AFTER THE COMPLETION OF THIS CAMPAIGN HAVE BEEN REPORTED AND ARE BEING EVALUATED AT THIS TIME.

THIS CAMPAIGN IS BEING PLACED ON HOLD TEMPORARILY IN THE INTEREST OF AVOIDING INCONVENIENCE TO OUR CUSTOMERS. ALSO, AT THIS TIME NO DECISION HAS BEEN MADE TO SEND OWNERS A NOTIFICATION LETTER ADVISING THEM OF THIS TEMPORARY CONDITION. WE ENCOURAGE ALL DEALERS TO MAINTAIN A LIST OF OWNERS WHO CONTACT YOU FOR THE COMPLETION OF THIS CAMPAIGN DURING THIS TEMPORARY PERIOD, SO THAT, WHEN IT IS RESOLVED YOU CAN SCHEDULE THESE OWNERS AND PROJECT A CARING IMAGE TO THEM.

ALL DEALERS WILL BE NOTIFIED WHEN TO RESUME PERFORMING AND/OR SCHEDULING OWNERS AND ANY OTHER DETAILS THAT MAY BE REQUIRED, FOR THE CAMPAIGN AS SOON AS IT IS RESOLVED.

PLEASE COMMUNICATE THIS INFORMATION TO ALL APPROPRIATE DEALERSHIP PERSONNEL.

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER." THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 CHEVROLET MOTOR DIVISION GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.