Hood Hold-Open Rod Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Raise and support the hood.
2. Remove the hood hold open rod (1).

The hood hold open rod (1) is bent at a right angle.

2.1. | Rotate the hood hold open rod (1) at the right angle.

2.2. | Pull the hood hold open rod (1) rearward to remove.

3. Remove the hood hold open rod retainer (2).

### Installation Procedure

1. Install the hood hold open rod retainer (2).
2. Install the hood hold open rod (1).

The hood hold open rod (1) is bent at a right angle.

2.1. | Rotate the hood hold open rod (1) at the right angle.

2.2. | Push the hood hold open rod (1) forward to fully seat in place.