Door Hardware Lubrication Description. Chevrolet PJJ 2000

For 1990-2009 cars

The mechanical components of the door assembly are lubricated during the assembly process. If additional lubrication is required, use the following lubricants:

Application | Type of Material | GM Part Number
--- | --- | ---
All Body Key Lock Cylinders | Multi-Purpose Lubricant or Synthetic SAE 5W30 Engine Oil | 12345120
Door Hinge Pins and Rollers | 30 Weight Engine Oil | --
Door Hardware Mechanisms (Excluding Lock Assemblies) | Lubriplate Spray-Lube A or Lubriplate Autolube A | 1052349 or 1502196