Rear Compartment Lid Latch Release Cable Handle Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the release handle cover.
2. Remove the remote release handle screws (3).
3. Remove the remote release handle nuts (1).
4. Remove the remote release cable (2) from the remote release handle (1).
5. Remove the remote release handle (1).

### Installation Procedure

1. Install the remote release handle (1).
2. Install the remote release cable (2) to the remote release handle (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the remote release handle screws (3) and nuts (1).

Tighten
Tighten the screws to 1 N·m (12 lb in).

4. Install the release handle cover.