Component Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Brake Pads

- Taper

0.15 mm

0.006 in

Front Brake Rotors

- Rotor Diameter

259.0 mm

10.197 in

- Installed Lateral Runout

0.08 mm

0.003 in

- Thickness Variation

0.013 mm

0.0005 in

Front Brake Rotor Thickness

- Minimum Thickness after Refinish

19.08 mm

0.751 in

- Discard Thickness

18.70 mm

0.736 in

- New Rotor

19.96 mm

0.786 in