Ignition Switch Replacement - On Vehicle. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the steering column trim covers. Refer to Steering Column Trim Cover Replacement.
3. Remove the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement-On Vehicle (With Key).
4. Remove the 2 TORX® head screws (2) from the ignition switch (3).
5. Remove the ignition switch (3) from the steering column (1).

### Installation Procedure

1. Install the ignition switch (3) to the steering column (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 2 TORX® head screws (2) to the ignition switch (3).

Tighten
Tighten the screws to 4 N·m (36 lb in).

3. Install the ignition lock cylinder. Refer to Steering Column Trim Cover Replacement.
4. Install the steering column trim covers. Refer to Ignition Lock Cylinder Replacement-On Vehicle (With Key).
5. Connect the negative battery cable.