SECURITY Indicator Always On or Flashing. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Instrument Cluster Diagnostic System Check? | Go to Step 2 | Go to A Diagnostic System Check - Instrument Cluster
2 | Test for a short to ground in the security indicator control circuit from the BCM to the IPC. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 4 | Go to Step 3
3 | Replace the instrument cluster (IPC). Refer to IP Cluster Replacement in Instrument Panel, Gauges and Console. Did you complete the repair? | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2