Door Striker Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the striker bolts (2).
2. Remove the washer (4).
3. Remove the spacer (3).
4. Remove the striker (1).

### Installation Procedure

1. Install the washer (4).
2. Install the spacer (3).
3. Install the striker (1).
4. Align the lock striker. Refer to Lock Striker Adjustment - Door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the striker bolts (2).

Tighten
Tighten the bolts (2) to 25 N·m (18 lb ft).