DTC P0108 Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage. Chevrolet PJJ 2000

For 1990-2009 cars
Engine Controls Components
Engine Data Sensors
OBD II Symbol Description Notice
Powertrain Control Module Connector End Views
Handling ESD Sensitive Parts Notice

### Circuit Description

The PCM uses the Manifold Absolute Pressure (MAP) sensor to control the fuel delivery and the ignition timing. The MAP sensor measures the changes in the intake manifold pressure which results from engine load (intake manifold vacuum) and the RPM changes; and converts these into a voltage outputs. The Powertrain Control Module (PCM) sends a 5 volt reference voltage to the MAP sensor. As the manifold pressure changes, the output voltage of the MAP sensor also changes. By monitoring the MAP sensor output voltage, the PCM knows the manifold pressure. A lower pressure (low voltage) output voltage will be about 1.0 to 1.5 volts at idle. While higher pressures (high voltage) output voltage will be about 4.5 to 4.8 volts at Wide Open Throttle (WOT). The MAP sensor is also used, under certain conditions, to measure barometric pressure, allowing the PCM to make adjustments for different altitudes.

### Conditions for Running the DTC

• | DTCs P0122 or P0123 is not set.

• | The Throttle Position (TP) sensor is less than 12 percent.

• | The vehicle speed sensor is less than 2 km/h (1 mph).

• | The engine run time is more than 20 to 40 seconds.

### Conditions for Setting the DTC

• | The MAP sensor is more than 82 kPa.

• | The above conditions are met for at least 1.25 seconds.

### Action Taken When the DTC Sets

• | The Malfunction Indicator Lamp (MIL) will illuminate after two consecutive ignition cycles in which the diagnostic runs with the fault active.

• | The Powertrain Control Module (PCM) will record operating conditions at the time the diagnostic fails. This information will be stored in the Freeze Frame and Failure Records buffers.

• | A history DTC is stored.

• | Coolant fan turns ON.

• | The PCM will substitute a fixed MAP value and use Throttle Position (TP) to control the fuel delivery (scan tool will not show defaulted value.)

• | The vehicle will operate in Open Loop when the vehicle is under 8 km/h (5 mph). The vehicle will operate in Closed Loop when the vehicle is over 8 km/h (5 mph).

### Conditions for Clearing the MIL/DTC

• | The MIL will turn OFF after three consecutive ignition cycles in which the diagnostic runs without a fault.

• | A history DTC will clear after 40 consecutive warm up cycles without a fault.

• | Use a scan tool to clear the DTCs.

### Diagnostic Aids

With the ignition switch ON and the engine stopped, the manifold pressure is equal to atmospheric pressure and the signal voltage will be high.

This information is used by the PCM as an indication of vehicle altitude. Comparison of this reading with a known good vehicle with the same sensor is a good way to check the accuracy of a suspect sensor. Readings should be the same +/- 0.4 volt.

DTC P0108 may set as a result of misfire. If misfire is present, repair the cause of misfire before using this table. The misfire counters may be used to determine which cylinder(s) is misfiring.

DTC P0108 may also set when attempting to start the vehicle that has run out of fuel.

Important: After repairs, use scan tool Fuel Trim Reset function to reset long term fuel trim to 128 (0 percent).

If a DTC P0108 is intermittent, refer to Symptoms or to the Manifold Absolute Pressure Sensor Output Diagnosis 2.4L for further diagnosis.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step simulates the conditions for a DTC P0107. If the PCM recognizes the change, the PCM, the 5.0 volt reference and the MAP sensor signal circuits are OK.

2. This step will determine if the DTC P0108 is the result of a hard malfunction or an intermittent condition.

3. This step looks for an open in the MAP sensor ground circuit.

4. When the MAP sensor signal circuit is shorted to battery voltage, the TP will display above 0 percent at all times and the A/C High Side will display high. The vehicle will also remain in Open Loop.

5. The MAP sensor vacuum source should only supply vacuum to the MAP sensor. Check the vacuum port for a restriction caused by casting flash.

6. Important: The Powertrain Control Module (PCM) uses a single internal 5.0 volt power supply to supply power to all the engine control components. If one component shorts its 5.0 volt reference circuit to ground or battery voltage, the other 5.0 volt reference circuits will also have a low or high voltage.

   Disconnect all of the sensors that use a 5.0 volt reference one at a time while monitoring the short on the 5.0 volt reference circuit. Replace any sensor that may have caused the short on the 5.0 volt reference circuit.

7. The replacement PCM must be programmed and the Crankshaft Position System Variation Learn procedure must be performed.

#### DTC P0108-Manifold Absolute Pressure (MAP) Circuit-High Voltage

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 | Start and idle the engine. Does the MAP voltage read more or equal to the specified value? | 4.0 V | Go to Step 3 | Go to Step 4

3

1. Turn OFF the ignition.
2. Disconnect the MAP sensor connector.
3. Turn ON the ignition, with the engine OFF.

Does the MAP voltage read the specified value or less?

1.0 V

Go to Step 5

Go to Step 6

4 | Operate the vehicle within the Freeze Frame conditions and Conditions for Running the DTC as specified in the supporting text. Does the MAP voltage read the specified value or more? | 4.0 V | Go to Step 3 | Go to Diagnostic Aids

5

1. Connect a test lamp to B+.
2. Probe the MAP sensor ground circuit.

Does the test lamp illuminate?

--

Go to Step 7

Go to Step 11

6

1. Turn OFF the ignition.
2. Test the MAP sensor signal circuit for a short to voltage.
3. If a problem is found, repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 15

Go to Step 12

7

1. Connect a DMM to ground.
2. Probe the 5.0 volt reference circuit.

Does the DMM display read near the specified value?

5.0 V

Go to Step 8

Go to Step 9

8

1. Turn OFF the ignition.
2. Inspect the MAP sensor vacuum source for the following conditions:

• | Plugged

• | Leaking

Did you find a problem?

--

Go to Step 10

Go to Step 12

9

Important:: The Powertrain Control Module (PCM) uses a single internal 5.0 volt power supply to supply power to all the engine control components. If one component shorts its 5.0 volt reference circuit to ground or battery voltage, the other 5.0 volt reference circuits will also have a low or high voltage.

1. Turn OFF the ignition.
2. Test the 5.0 volt reference circuit for a short to battery voltage.
3. If a problem is found, repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 15

Go to Step 13

10 | Repair the vacuum source as necessary. Did you complete the repair? | -- | Go to Step 15 | --

11

1. Turn OFF the ignition.
2. Test/Inspect for the following conditions in the MAP sensor ground circuit:

• | Open circuit

• | Poor connections

3. If a problem is found, repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 15

Go to Step 13

12

1. Inspect the MAP sensor ground circuit for poor connections.
2. If a problem is found, repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 15

Go to Step 14

13 | Important:: The replacement PCM must be programmed. Refer to Powertrain Control Module Replacement/Programming Replace the PCM. Refer to Powertrain Control Module Replacement . Did you complete the replacement? | -- | Go to Step 15 | --
14 | Replace the MAP sensor. Refer to Manifold Absolute Pressure Sensor Replacement . Did you complete the replacement? | -- | Go to Step 15 | --

15

1. Use a scan tool to clear the DTCs.
2. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC reset?

--

Go to Step 2

System OK